#

# Meteor M-N2 and N2-2 Satellite Operational Status

## Meteor-M N2:
#### Frequency | #### SymbolRate | #### LRPT Status
137.100MHz | 72.000K | On
#### APID 64 | #### APID 65 | #### APID 66
On | On | On
#### APID 67 | #### APID 68 | #### APID 69
Off | Off | Off
## Notes: Visible Channels 1, 2, 3. Active Channels: Channel 1 Visible (0.5 0.7 Âµm; APID64), Channel 2 Visible (0.7 1.1 Âµm; APID65), Channel 3 Visible (1.6 1.8 µm; APID66). 25.03.2021 Switched to RGB-123 mode for this season, RGB-125 back in September. 16.05.2021 Meteor M-N2 sent channel-by-channel pictures and there are line failures in the second channel. MSU was restarted all working fine.

## Meteor-M N2-2:
#### Frequency | #### SymbolRate | #### LRPT Status
137.900MHz | 72.000K | Off
#### APID 64 | #### APID 65 | #### APID 66
Off | Off | Off
#### APID 67 | #### APID 68 | #### APID 69
Off | Off | Off
## Notes: Visible/IR Channels 1, 2, 5. Active Channels: Channel 1 Visible (0.5 0.7 Âµm; APID64), Channel 2 Visible (0.7 1.1 Âµm; APID65), Channel 5 Infrared 10.5 ± 0.50 - 11.5 ± 0.50 µm; APID68, 19 December Telemetry analysis and an attempt to stop rotation are being carried out. 20 December Meteor M-N2-2 is stabilized, work is ongoing with the satellite. 24 December Orbit dropped with 1KM on Dec 18, 01:09 UTC due Depressurization from possible collision. Depressurization caused gas that was inside and used for heat transfer to leak out. Resulting in some devices onboard overheating, while others did stop working. Batteries are working under harsh thermal conditions. Experts analyzing MSU-MR images during the incident to confirm collision. Roscosmos Official News 26 December X-Band MSU-MR Onboard Storage Memory Transmission (Not Live) January 2020 There will be only short-term power-ups in the radio visibility zone, and the battery life will be reduced tenfold. Of particular concern are the batteries they are very quickly overheated and switching from regular to backup. Unfortunately the power supply features do not allow the 137MHz transmitter to be used in abnormal power, mode (from solar panels) which is used now although technically it is working fine. There will be no LRPT Transmission's anymore..