@import url(../pmwiki/pub/skins/sinorca/basic.css); @import url(../pmwiki/pub/skins/sinorca/layout.css); @import url(../pmwiki/pub/skins/sinorca/sinorca.css);

2021-01-31 16:07:24

- RSS
- ATOM
- All recent changes

# r00t.cz

- Home
- Login
- Search

- View
- Edit
- History
- Print

## S-Band satellite signals

Page: Sats.S-Band - Last Modified : Sun, 08 Feb 15

.txt { padding-left:10px;font-family:Courier; } .top { background-color: rgb(0, 51, 153);padding-left:10px } .tim { background-color: rgb(0, 51, 153);color:#eee; } .tab { font-family: Arial;font-size: 15px;background-color:#eee;font-weight:bold; } .hdr2 { width: 100%;font-size:15px; } .hdr2 tr td { padding-right:10px;font-family: Courier;color:#eee;} .hdr2 tr td:first-child { font-size: 18px;font-family:Arial;color:#fff} .txth { text-align: right;font-size:15px;color:#888; }

2250.0MHz OCEANSAT-2 | (NORAD 35931)
| 2013-11-09
MODULATION | PM + 32000Hz subcarrier (4000Bd DBPSK) |
FRAMING | 1024bit frame, poss. sync 0xACCA1F11
DATA/ID | custom multiplexed/framed data

2254.8MHz BEIDOU-IGSO3 | (NORAD 37384)
| 2013-11-08
MODULATION | PM + 65536Hz subcarrier (2048Bd DBPSK) |
FRAMING | CCSDS 2048bit frame, unscrambled
DATA/ID | CCSDS V2 0x123 = KOMPSAT-3 ??? no assigned ID ???

2256.0MHz BEIDOU-M4 | (NORAD 38251)
| 2013-11-08
MODULATION | PM + 65536Hz subcarrier (2048Bd DBPSK) |
FRAMING | CCSDS 2048bit frame, unscrambled
DATA/ID | CCSDS V2 0x144 = (FMBPrime) ??? no assigned ID ???

2262.4MHz CLOUDSAT | (NORAD 29107)
| 2013-11-09
MODULATION | PM + data (direct, no subcarrier, 524288Bd 1/2 viterbi) |
FRAMING | Custom telemetry, 4096bit frame, poss. sync: 0x06DE5194
DATA/ID |

2264.6MHz Eutelsat 12 West A | (NORAD 27508) (GEO@12.5°W)
| 2013-11-09
MODULATION | PM + 32768Hz subcarrier (8192Bd BPSK 1/2 viterbi, unscrambled) |
FRAMING | CCSDS 2072bit frame, 1 RS check block
DATA/ID | CCSDS V1 0x0A4 = ATLANTICBIRD1

2266.3MHz Yaogan-8 | (NORAD 36121)
| 2013-11-08
MODULATION | PM + 65536Hz subcarrier (8192Bd DBPSK) |
FRAMING | 2048bit frame, sync 0xFAF320
DATA/ID | basic tlm + encrypted block

2273.5MHz Haiyang-1B | (NORAD 31113)
| 2013-11-09
MODULATION | PM + 65536Hz subcarrier (4096Bd DBPSK) |
FRAMING | 1024bit frame, sync 0xEB90
DATA/ID |

2276.4MHz TX-1 | (NORAD 37874)
| 2013-11-09
MODULATION | PM + 65536Hz subcarrier (4096Bd DBPSK) |
FRAMING | 512bit frame, sync 0xEB90
DATA/ID |

2296.6MHz Yaogan-6 | (NORAD 34839)
| 2013-11-08
MODULATION | PM + 65536Hz subcarrier (4096Bd DBPSK) |
FRAMING | 2048bit frame, sync 0xFAF320
DATA/ID | 13 bytes of basic tlm + 208 bytes of encrypted data

2274.3MHz SMAP | (NORAD 40376)
| 2015-02-08
MODULATION | 4588Bd DBPSK |
FRAMING | 10232bit CCSDS frame with 5 blocks of RS
DATA/ID | HDR v2 S/C ID 0xCD (registered as "SMAP" in SANA) Basic telemetry on VC0/APID10, VC63 used for padding. Padding contains this nice message!

All content on this webpage is published for personal use only.
You are using any software downloaded from this page at your own risk. Some software may be illegal to use in your country.

© r00t 2009-2012 (email: r00t@<this domain>)