  TEST MONITOR   1.1
-------- r00t 2002 ----


1. ON/OFF
2. SERVING CELL
3. NEIGHBOUR CELLS
4. STATISTICS
5. POWER OFF
6. MEM USAGE
7. CAUSE CODES


1. ON/OFF
Disable or enable all other functions.


2. SERVING CELL

ChanNW Signal
CellID SIMx:x
currC1 00 DSCxxx
LAI ctr op cell
TXPWRxx RXAMxxx

ChanNW ......... current BTS channel
Signal ......... RX level in dBm
CellID ......... CellID - CID (hex)
currC1 ......... Value of the path loss criterium (C1)
ctr op ......... Country and operator code
cell ........... Local Area Code - LAC (hex)
TXPWRxx ........ TX power level
RXAMxxx ........ Minimum BTS power level

3. NEIGHBOUR CELLS

.CH..RX.C1.C2.NB
Schn rx c1 c2   - Current BTS
1chn rx c1 c2   - ch1
2chn rx c1 c2   - ch2
3chn rx c1 c2   - ch3
4chn rx c1 c2   - ch4
5chn rx c1 c2   - ch5
6chn rx c1 c2   - ch6


Xchn ........... BTS channel
RX ............. RX level in dBm (without -)
C1 ............. Path loss criterium (C1)
C2 ............. Cell reselection criterium (C2)


4. STATISTICS

Hxxxxx MHxxxxx
SYcntr MSYxxxx
MTCxxxx MOCxxxx
DCxxxx CSFxxxx

SYcntr ......... SYSTEM counter


5. POWER OFF

MinXXX VoltNDDD
TempCCCC PSxxxx
Slpxxxx 32kxxxx
SDC: xxxxxx
Lxxxx
CVoltXXX Mxx
FTxx HSxx
Voltage History
Idle   TX
xxxx   x
xxxx   x
xxxx   x
xxxx   x

MinXXX ......... Timer, startted when phone is turned on
Volt ........... Battery voltage in mV
TempXXXX ....... Temperature of battery in 5C steps
32Kxxxx ........ 32k counter
SDC: xxxxxx .... Last non-normal exitcode
CVoltXXX ....... Charging voltage in mV
Voltage History: Show last 4 values of battery voltage
                 in idle mode and during TX



6. MEM USAGE

[PROCESS NAME] [USED PROCESS MEMORY]
Process name followed by percent usage of it's memory.
Press Green button to reset values to 0.

7. CAUSE CODES

Cause Codes:
CC: valC cnt:ctC
MM: valM cnt:ctM
RR: valR cnt:ctR

Information about reasons for call clearing

valC ........... CC cause value, see section 10.5.4.11/GSM 04.08
ctC ............ CC error counter
valM ........... MM cause value, see section 10.5.3.6/GSM 04.08
ctM ............ MM error counter
valR ........... RR cause value, see section 10.5.2.31/GSM 04.08
ctR ............ RR error counter
