# X-Band Beacon Summary

UHF-Satcom.com - European X-Band beacon guide

Satellite | Location | Frequency | Pol | Modulation | FFT
--- | --- | --- | --- | --- | ---
WGS-F2 | 60.0 East | 7600.000 | LHCP | TT&C |
DSCS3-12 | 57.0 East | 7600.000 | LHCP | TT&C |
DSCS3-12 | 57.0 East | 7604.706 | LHCP | TT&C |
Skynet 5D | 53.0 East | 7492.200 | LHCP | Beacon / Continuous carrier |
Syracuse 3A | 47.0 East | 7284.000 | LHCP | Beacon / Continuous carrier | No signals detected
Syracuse 3A | 47.0 East | 7720.000 | LHCP | DSSS TT&C | No signals detected
Syracuse 3A | 47.0 East | 7737.500 | LHCP | TT&C Beacon | No signals detected
Turksat 2A Turksat 3A | 42.0 East | 7410.000 | LHCP | Beacon / Continuous carrier |
Nato 4B | 35.0 East | 7345.000 | LHCP | Beacon / Continuous carrier | No signals detected
Nato 4B | 35.0 East | 7587.500 | LHCP | Beacon / Continuous carrier | No signals detected
Skynet 4E | 32.5 East | 7249.995 | LHCP | Beacon / Continuous carrier |
Skynet 4E | 32.5 East | 7372.700 | LHCP | TT&C |
Skynet 4E | 32.5 East | 7397.500 | LHCP | TT&C |
UFO-2 | 29.2 East | 7260.000 | LHCP | TT&C |
Xtar-EU | 29.0 East | 7251.000 | LHCP | Beacon / Continuous carrier |
DSP-F18 | 20.7 East | 7293.700 | LHCP | FHSS |
Sicral-1 | 16.1 East | 7500.000 | LHCP | TT&C |
ComSatBW2 | 13.3 East | 7515.000 | LHCP | TT&C |
Sicral-1B | 11.8 East | 7305.000 | LHCP | TT&C |
Sicral-1B | 11.8 East | 7405.000 | LHCP | TT&C |
Skynet 5A | 6.0 East | 7494.000 | LHCP | TT&C |
Skynet 4C | 1.6 West | 7331.500 | LHCP | TT&C |
Syracuse 3B | 5.2 West | 7705.000 | LHCP | TT&C |
WGS-F3 | 12.0 West | 7600.000 | LHCP | TT&C |
Skynet 5C | 17.9 West | 7492.200 | LHCP | TT&C |
SpainSat | 30.0 West | 7250.516 | LHCP | TT&C |
SpainSat | 30.0 West | 7749.504 | RHCP | TT&C |
Skynet 4F | 34.0 West | 7250.000 | LHCP | Beacon / Continuous carrier |
Skynet 4F | 34.0 West | 7540.000 | LHCP | Beacon / Continuous carrier |
DSP-F17 | 52.3 West Inc | 7293.700 | LHCP | FHSS |
DSCS3-14 | 52.5 West | 7600.000 | LHCP | TT&C |
DSCS3-14 | 52.5 West | 7604.704 | LHCP | TT&C |